/******************** (C) COPYRIGHT 2014 STMicroelectronics ********************
* File Name          : readme.txt
* Author             : MCD Application Team
* Version            : V1.4.0
* Date               : 10/20/2014
* Description        : read me file for Virtual COM Port driver 
********************************************************************************
* THE PRESENT SOFTWARE WHICH IS FOR GUIDANCE ONLY AIMS AT PROVIDING CUSTOMERS
* WITH CODING INFORMATION REGARDING THEIR PRODUCTS IN ORDER FOR THEM TO SAVE TIME.
* AS A RESULT, STMICROELECTRONICS SHALL NOT BE HELD LIABLE FOR ANY DIRECT,
* INDIRECT OR CONSEQUENTIAL DAMAGES WITH RESPECT TO ANY CLAIMS ARISING FROM THE
* CONTENT OF SUCH SOFTWARE AND/OR THE USE MADE BY CUSTOMERS OF THE CODING
* INFORMATION CONTAINED HEREIN IN CONNECTION WITH THEIR PRODUCTS.
*******************************************************************************/

Last version 
***************
       - V1.4.0 - 10/20/2014
Supported OS
***************

       + Windows 98SE, 2000, XP, Vista, Seven, 8.x (x86 & x64 Windows platforms)
 
Contents
***********
       + VCP_V1.4.0_Setup.exe            : Setup file to Copy required files
	   + version.txt                     : History of versions
	   + readme.txt                      : This file

How to use 
***************

       1- Uninstall previous versions (Start-> Settings-> Control Panel-> Add or remove programs)
       卸载以前的版本

       2- Run your "VCP_V1.4.0_Setup.exe" 
       管理员模式运行"VCP_V1.4.0_Setup.exe" 
	   
       3- Go to Your installation directory - Example, C:\Program Files (x86)\STMicroelectronics\Software\Virtual comport driver
       找到"VCP_V1.4.0_Setup.exe" 解压出来的usb驱动，比如下面的路径：C:\Program Files (x86)\STMicroelectronics\Software\Virtual comport driver
	   
       4- Go to Your OS version directory ([Win7] or [Win8])
			+ Then :
				- Double click on dpinst_x86.exe if you are running a 32-bits OS version
				- Double click on dpinst_amd64.exe if you are running a 64-bits OS version
			+ Follow the instructions.

       根据你的操作系统双击dpinst_x86.exe(32bit系统)或者dpinst_amd64.exe(64bit系统)

       5-注意：如果是win10系统会自动安装驱动，如果是xp,win7,win8需要手动安装驱动，如果电脑操作系统不是官方原版，而是ghost或者精简系统
       可能会遇到安装失败的问题，可以在网络上搜索"ST 虚拟串口驱动安装失败"获取解决方式，下面是一个解决案例：
       缺少usbser.sys(c:\windows\system32\drivers)，mdmcpq.inf(c:\windows\inf)这2个文件,去网络上面下载对应操作系统的这两个文件，mdmcpq.inf修改下就可以，
       注释掉[FakeModemCopyFileSection]节点下的usbser.sys：
       [FakeModemCopyFileSection]
       ;usbser.sys    


******************* (C) COPYRIGHT 2014 STMicroelectronics *****END OF FILE******